# XENTEK Cascade v3.6.2

- Corrects spoken cell deviation for parallel battery banks.
- Reports the largest deviation within one battery module.
- No longer compares a low cell from one battery with a high cell from another.
- Adds a Full status report button to the public dashboard.
- Retains the numeric-speech and PV-production improvements from v3.6.1.
